Contents

[Overview 2](#_Toc12265738)

[Hardware and Raspberry Pi 2](#_Toc12265739)

[Camera Port 2](#_Toc12265740)

[USB Ports 2](#_Toc12265741)

[GPIO Pins 2](#_Toc12265742)

[Installing the operating system 3](#_Toc12265743)

[Setting up python 4](#_Toc12265744)


[Running the program 5](#_Toc12265745)

[Program overview 6](#_Toc12265746)


[Class Structure Overview 7](#_Toc12265747)

# Overview:

## Hardware and Raspberry Pi

The raspberry pi is a microcomputer that is used in this project as the logical controller. The raspberry pi is equivalent to a normal computer in that it has its own operating system, multithreading, and a motherboard. In figure 1, you can see the various inputs and outputs of the raspberry pi. Note that the raspberry pi has built in Bluetooth, and wireless capabilities.

### Camera Port

The raspberry pi has a dedicated camera port slot. This allows for high speed transfer of data that a normal USB port cannot achieve. Most attachments to the top of the raspberry pi (called hats) has a slot to pass the camera cord through to allow a camera to be used with the module.


### USB Ports

The raspberry pi comes with four USB type A ports for data transfer. Additionally, the raspberry pi comes with a single 5V micro USB port to power the raspberry pi. Note, the batteries used in this robot supply roughly 3.5 amps. The raspberry pi takes 1 amp to run, not including the power drain through USB ports. While the current sensors used through USB are compatible with the amperage limits, if more amperage than what is supplied to the raspberry pi is used, an externally powered USB hub would be required

### GPIO Pins

See figure 2 for the pinout diagram. The GPIO pins send raw data through multiple different types of ports and configurations. The simplest way to use the GPIO pins for testing is with a breadboard. This allows for wires to be inserted into the breadboard for easy testing without soldering. Note that the I2C ports can be parallel ports, this means that multiple devices can use the I2C ports. All other ports can only be accessed by one device at a time.

# Installing the Operating System

Because the SD card in the raspberry pi may need to be replaced, you may need to reinstall the operating system back onto the raspberry pi.

## Parts Needed

1. Raspberry Pi
2. MicroSD card (At least 8gb)
3. MicroSD to USB converter
4. External computer
5. Mouse
6. Keyboard
7. Monitor
8. HDMI cord

## Installing the ISO

1. Download the raspbian ISO [here](https://www.raspberrypi.org/downloads/raspbian/). Select the desktop version with recommended software
2. Download and install Win32DiskImager [here](https://sourceforge.net/projects/win32diskimager/). Launch the program. It should look like figure 3
3. Select the ISO file you downloaded
4. Keeping all the default settings, press write
5. The program will display a warning message, saying the Micro-SD card will be wiped, press continue
6. Allow the program to mount the ISO onto the Micro-SD card.

## Installing the operating system

1. Insert the micro SD card into the micro SD slot on the back of the raspberry pi
2. Connect a power source to the raspberry pi, it should boot up after a few minutes to the main screen.

## Updating the operating system

In order to update the operating system (which should be done on first startup):

1. Run:

sudo apt-get update  
sudo apt-get dist-upgrade

## Logging in

1. The default login credentials are:
2. Username: pi
3. Password: Password01

## Accessing the Raspberry Pi remotely through another computer

While connecting with a mouse keyboard and monitor works, a simple and portable solution would be to login using VNC viewer

1. On the console run:


sudo apt-get update  
sudo apt-get install realvnc-vnc-server

IP Address:

sudo raspi-config

1. Navigate to interfacing options > vnc and ensure it is enabled
2. On the raspberry pi console run:

sudo ip addr show

1. Write down this ip address for later use
2. On the remote computer (Windows):  
   [Download VNC viewer](https://www.realvnc.com/en/connect/download/viewer/)  
   Input the ipaddress into the search bar and press enter to establish a connection

# Setting up python and git

Note: Both python 2 and python 3 are installed by default on Raspbian. For this project we are using python 3

## Verify installation

1. Open a console window
2. Type these two commands to ensure installation:   
   python3 -–version  
   pip –-version  
   git
3. These three should return information. If an error message is received, they must be installed

## Set up a git repository

In order to setup a place to download the program and libraries, a git repository must be set up.

1. Using ls (to show files) and cd (to change directory, or folder) in the console window, navigate to the desktop
2. Use:  
   mkdir git  
   To create a folder to store all github projects. Navigate into this folder
3. Use:  
   sudo git clone github.org  
   Where github.org is the link to the git project available for export on the project’s website  
   The link should be: <https://github.com/danielsmith1313/Robot.git>
4. The entire library should now be downloaded.

## Retrieving changes from a git repository

While we have the code now, it is much easier to edit the code externally and pull the changes

1. Navigate to the project directory under the git directory
2. Type: sudo git pull
3. The git repository should be updated

## Installing python dependencies

1. Navigate to the requirements.txt folder under the git project
2. For each line in this file type:

sudo pip3 install filename

# Running the program

# Program overview

# Class Structure Overview